**USER MANUAL**

[1. Running Environment](#_Toc8123)

[2. Software Installation](#_Toc4540)

[2.1 Client Downloading](#_Toc20124)

[2.2 Client Setup](#_Toc11075)

[3. Software Activation and Downloads](#_Toc14243)

[3.1 Software Activation](#_Toc22264)

[3.2 Software Download](#_Toc26956)

[3.3 Software Management](#_Toc26690)

[4. Software Introduction](#_Toc29886)

[4.1 IDUTEX Store](#_Toc29091)

[4.2 Diagnosis Service System (DSS)](#_Toc6295)

[4.2.1 Features](#_Toc31936)

[4.2.2 Vehicle Coverage](#_Toc28519)

[4.2.3 System Coverage](#_Toc31612)

[4.2.4 Function Coverage](#_Toc9931)

[4.3 Settings](#_Toc803)

[4.3.1 System info](#_Toc11389)

[4.3.2 Unit](#_Toc10680)

[4.3.3 Search Engine](#_Toc26845)

[4.3.4 Run Mode](#_Toc24287)

[4.3.5 OS Versions](#_Toc6839)

[4.3.6 Languages](#_Toc9474)

[4.3.7 About US](#_Toc18011)

[4.4 DTC Query](#_Toc29848)

[4.5 Dictionary](#_Toc31288)

[4.6 Example](#_Toc8895)

[4.6.1 Communication](#_Toc32161)

[4.6.2 Read ECU Information](#_Toc11655)

[4.6.3 Read DTCs](#_Toc25188)

[4.6.4 Erase DTCs](#_Toc9110)

[4.6.5 Data List](#_Toc30800)

[4.6.6 Active Test](#_Toc18974)

[4.6.7 Special function](#_Toc23025)

[4.7 Screenshot](#_Toc31536)

[4.8 Save](#_Toc17404)

[4.9 Screen recording](#_Toc18415)

[4.10 Data Playback](#_Toc13633)

[4.11 Diagnose Function List](#_Toc1340)

[4.12Feedback](#_Toc805)

[4.13Data Management](#_Toc24266)

[4.13.1 Image Management](#_Toc12015)

[4.13.2 APP Management](#_Toc11191)

[4.13.3 Video Management](#_Toc27241)

[4.13.4 Report Management](#_Toc22821)

[4.14 User Management](#_Toc28328)

[4.15 Quick Support](#_Toc8810)

[5. Products Website](#_Toc7671)

[6. Warranty](#_Toc19393)

# 1. Running Environment

* Hardware Environment:

Memory: more than 1GB

Communication port: Bluetooth

* Software Environment:

Based on Android4.4 above the smart phone system

# 2. Software Installation

## 2.1 Client Downloading

Access to website: http://www.IDUTEX.com, and download “**VPECKER E4 EN Setup V**x.x”（xx represents the version number）.

## 2.2 Client Setup

Click“VP\_E4\_EN\_V4.4.apk” and run VPECKER E4.apk:



Please click “Install”.



Installing...


|  |
| --- |
| 安装2安装1 |

VPECKER Bluetooth diagnostic service system installs successfully.

# 3. Software Activation and Downloads

## 3.1 Software Activation


At first, please keep network working. Run VPECKER E4 APP, then click “IDUTEX Store” to get applications.



Please click “OK”.


|  |
| --- |
| 主界面0主界面1 |

Please click “IDUTEX Store”.




Please enter the S/N number and password get from the envelope, and then click “”.






Please click “”.



If the product is not activated, please click “Yes”.



Please input your information, the Email address and country are required, and then click “Activate”.

.

Note:

Your email address must be real in order to get the activated link and the further better service from the manufacturer. The software update reminder and the new product release information will be sent to your email.

If you do not receive the activation email, please add"support@idutex.com" to the white list of your mailbox and try the activation process again.

Company name: company name must be filled in and the length is within 250 characters.

Country: please choice your country in the list.

|  |
| --- |
|  |

Please click the link to get the confirmation from the manufacturer.

|  |
| --- |
|  |

## 3.2 Software Download

After the activation, please login the IDUTEX store again, and get the APPs upgrade.

|  |
| --- |
| 主界面0登录商城1 |

Please, click “” to download the software.

There are three modes for downloading, one by one and one-click. It may take a long time to download all the software, due to customers’ network speed reason.please wait patiently.

|  |
| --- |
| 商城1车型选择 |

Please, click the button“” to select vehicle software you want to download, and click the button “” to download one by one.

Or click the button“” to select all modle, and click the button “” to do one-click download.

## 3.3 Software Management

Users can delete vehicle software here. You can delete one by one or all-selected delete.

|  |
| --- |
| APP1App2 |

Please, click the button“” to select the software you want to delete, and click the button “” to delete.

Or click the button“” to select all Apps, and click the button “” to do one-click delete.

# 4. Software Introduction

Run VPECKER E4，The screen will show:

|  |
| --- |
| 主界面0主界面1 |

## 4.1 IDUTEX Store

Features

● Automatic Wi-Fi updates available in new software releases by smart upgrade mode.

● Wi-Fi internet capability allows for wireless access throughout the workshop.

● Extremely easy-to-use with touch-screen operation and intuitive operation in the Android.

|  |
| --- |
| 商城1商城3 |

## 4.2 Diagnosis Service System (DSS)

### 4.2.1 Features

● Complete function capability including live data, ECU programming and so many others.

● Unparalleled OBDII functionalities-support ALL 5 OBDII protocols and ALL 10 test modes.

● Can check out the year and model of the vehicles automatically and quickly.

● Android 4.4 above operating system allows for more stable performances, better compatibility and expandability.

### 4.2.2 Vehicle Coverage

**Europe:**

Abarth, Alfa, Aston, Audi, Bentley, Benz, Bmw, Bugatti, Citroen, Dacia, Ferrari, Fiat, Fordeu, Jaguar, Lamborghini, Lancia, Landrover, Maserti, MINI, Opel, Peugeot, Porsche, Renault, SAAB, Seat, Skoda, Smart, Vauxhall, Volvo, VW.

**Asia:**

Acura, Asiagm, Daewoo, Daihatsu, Honda, Hyundai, Infiniti, Isuzu, KIA, Lexus, Mazda, Mitsubishi, Nissan, Perodua, Proton, Ssangyong, Subaru, Suzuki, Toyota.

US domestic:

Chrysler, Ford, Gm, Jeep, Scion.

**Australia:**

Holden, Ford (Australia).

**China:**

BYD, Changan, Changhe, Chery, Emgrand, Englon, Foton, Geely, Gleagle, GWM, HBSH, Huachen, Lifan, Wuling, Yuan.

**OBDII:**

Abarth, Alfa, Aston, Audi, Bentley, Benz, Bmw, Bugatti, Citroen, Dacia, Ferrari, Fiat, Fordeu, Jaguar, Lamborghini, Lancia, Landrover, Maserti, MINI, Opel, Peugeot, Porsche, Renault, SAAB, Seat, Skoda, Smart, Vauxhall, Volvo, VW.

### 4.2.3 System Coverage

**Drive:**

CDI, HFM, ECM, ETC, FTC, FCVT, GRM, ACS, ESM, DF, VG Transfer case, VGS, FSCU, HAQ, HSG, IFI, ISM, PTCU, SCR, SEQ, SGR, etc.

**Chassis:**

ABC, ABR, ABS, ADS, AIRMATIC, AMG DRVU, ASR, BAS, DIF, DTR, EFB, EHPS, ENR, EPS, ES, ESP, RBS, SBC, SPS, TPC, VP, etc.

**Body:**

AAG, AAM, Airbag, ACL , AGS, AHE, AIRSCARF, AIS, ALWR, AMG DRVU, APS, ASD, ATA, BCG, BCM, BS, CCM, CGW, CL, CRN, DAS, DC, EAM, EDW, EIS, EZS, GTO, HBF , HKS, HLCMHRA , IRS, KE, KG, LCP, Lighting, MSC, OBF, OCP, SAM , PSD, PSE, PTS, Rear SAM, RFL , RLS, RS, RVC, SAM, SCCM, SD, SDE, SEM, SG, SRS, SVMCM, UCP, VBF, VR, WBS, WSP , WSS, XALW , etc.

Seats and Doors AIRSCARF, CL, DCM, DCU, DS, DSP, ERA, ESA, ESD, HRS, HS, LAE, LDCA, MKL, MKS, OSB, PESA, PPAMKS, PWC, RCM, REDC, ESE, RWT, STL , SVS, TLC, etc.

**Air Conditioning:**

Air conditioning, Automatic heater, C-AAC, HBF, HEAT/TAC, HSW, HZR, KBE, PTC, REAR, SG-EM, STH, TAC, ZHE Auxiliary heater, ZHZ Heater booster, etc.

**Information and Communication：**

AGW, APS, ASSYST, AUDIO, AVE, BA, CDC, CD changer, CM, CTEL, DN, Drive Kit Plus, DSI, DTC, GPS box, HFS, IC, ICM, KOMO, Left rear screen, MB Portal, E-mail, Mercedes, MIF, MTCO, NAV, NSA, PTS, Radio, RFK, SCM, TB, TPAD, UC, UHI, VCS, WSP, ZAN, etc.

**Recreational Vehicles:**

Warm air stationary heater, Eletcrohydraulic pop, Sliding roof in pop, Voltage supply, Interior lighting, etc.

**Special Bodies:**

PSM, Kerstner, PSM, etc.

**Driver Assistance System:**

360 camera, DTR, IRS, KAB, MFK, NSA, PARK, PTS, RFK, SG, TPM, etc.

### 4.2.4 Function Coverage

Read Version Information, Read DTC, Clear DTC, Data Stream, Actuation Test, Data Stream, Actuations, Read freeze frame data,EPB, TPMS, ABS BLEEDING, DPF, EPS, BATTERY, INJECTOR, Read/Write VIN, Control unit adaptations, Throttle adaptations, Air bleeding, Level calibration, Theft alarm Reset, Key programming, Oil change, Idle speed learning, Idle speed Adjustment, Ignition timing adjustment, Camshaft timing control learning, Maintenance functions, ECU Initial startup, ECU initialization, etc.

## 4.3 Settings

### 4.3.1 System info

Automatically identify Vpecker and Vpecker version information, when connection has problem (Wi-Fi or Bluetooth), and it can’t read Vpecker Hardware version, usually, it shows as “Unknown” or “---”; If the connection is OK, it shows hardware version. As the picture shows:

|  |
| --- |
| Settings版本信息1_副本 |

### 4.3.2 Unit

Unit switch between Metric and Imperial system:

|  |
| --- |
| 图片1unit |

### 4.3.3 Search Engine

This feature is based on different browser on your mobile APP and you can set different search engine.

|  |
| --- |
| 图片1search engine |

### 4.3.4 Run Mode

When VPECKER E4 is not connected, you can simulate the operation of the vehicle through the operating mode, as shown in the following figure:

|  |
| --- |
| 图片1run mode |

### 4.3.5 OS Versions

If there i a new version, it can automatically prompt to update.

|  |
| --- |
| 图片1os versions |

### 4.3.6 Languages

Choose the language you need, as the picture shows:

|  |
| --- |
| 图片1语言 |

Language coverage: Supporting more 22 languages, including English, Japanese, German, Russian, French, Italian, Spanish, Portuguese, Polish, Turkish, Dutch, Hungarian, Korean, Czech, Arabic, Indonesian, Persian, Thai, Vietnamese, Finnish, Swedish, Romanian, etc.

### 4.3.7 About US

|  |
| --- |
| *Settingsabout us* |

## 4.4 DTC Query

|  |
| --- |
| 主界面0故障码查询0 |

DTC query function is a DIY function, users can query, modify and create OBD DTCs by themselves requirement in local DTCs, and users can synchronize to IDUTEX company cloud server through the internet too.

|  |
| --- |
| DTC Querydtc query 2 |

It supports both DTC query offline and online.

## 4.5 Dictionary

You can use this function to query automotive terms, abbreviations or commonly used English sentences.

|  |
| --- |
| dictionary0dictionary1 |

## 4.6 Example

### 4.6.1 Communication

Please connect VPECKER E4 with the car. After connection, the indication light turn on red.

Please check the connection of Bluetooth, if connect successfully, the indication light will turn to blue.

Run the VPECKER and start to diagnose.

Take BMW as an example:

|  |
| --- |
| Diagnosecopytoqq |
| copytoqqcopytoqq |
| copytoqqcopytoqq |
| copytoqqcopytoqq |
| copytoqqcopytoqq |

### 4.6.2 Read ECU Information

|  |
| --- |
| copytoqqcopytoqq |

### 4.6.3 Read DTCs

|  |
| --- |
| copytoqqcopytoqq |

### 4.6.4 Erase DTCs

|  |
| --- |
| copytoqqcopytoqq |

### 4.6.5 Data List

|  |
| --- |
| copytoqqcopytoqqcopytoqqcopytoqq |

Click the button  to start data recording, until to click the button  to stop recording:

|  |
| --- |
| copytoqq |

Please chick the  button to select the data stream you want, click the  button, vertical screen will show the dynamic effect of data stream.

|  |
| --- |
| Diagnose 32copytoqq |

Click the  button, horizontal screen will display dynamic effects of superimposed waveform for data stream.

|  |
| --- |
| Diagnose 34 |

Click the  button to change the waveform line color, you can select the color you like and click "OK" button.

|  |
| --- |
| Diagnose 35 |

### 4.6.6 Active Test


|  |
| --- |
| copytoqqcopytoqq |

### 4.6.7 Special function

|  |
| --- |
| copytoqqcopytoqq |
| copytoqqcopytoqq |
| copytoqqcopytoqq |
| copytoqqcopytoqq |


## 4.7 Screenshot

Captures, saves and prints screenshots anytime and anywhere.



The screenshot files save at the path:

My fileI/ Internal storage/IDUTEX/U3/UserData/Screenshots



## 4.8 Save

Using the saving function to generate the corresponding diagnostic report document for the vehicle diagnostic data, it greatly facilitates the diagnosis and management of the diagnosis and management of the diagnostic data.

Click the button  to save the diagno stic report .

|  |
| --- |
| Diagnose 28 |

Click the button  to view the diagnostic report , as the picture show:

|  |
| --- |
| reportcopytoqq |

## 4.9 Screen recording

Click the button  to start the screen recording, click  again to stop the screen recording. Use the function to record VPECKER operation and generate the appropriate video files, The video can be checked in video management.

|  |
| --- |
| copytoqq |

## 4.10 Data Playback

You can quickly browse the video of the diagnostic data you have recorded here.

|  |
| --- |
| copytoqqcopytoqq |

## 4.11 Diagnose Function List

Click the  button to open the vehicle function list, you can quickly understand the supported models, systems and functions. As shown below:

|  |
| --- |
| Diagnosecopytoqq |

## 4.12Feedback

The information of diagnostic software problems can be uploaded to the manufacture by this function. It helps the engineers to fix the bugs quickly.

|  |
| --- |
| feedback0feedback1 |

NOTE: With \* information is required; the attachments size cannot exceed 8MB.

## 4.13Data Management

### 4.13.1 Image Management

Here you can browse or delete the Images.

Click the image to browse the picture. Click the button  to delete the picture.

|  |
| --- |
| imagesimges 1 |

### 4.13.2 APP Management

Users can delete the diagnostic software here, one by one or all-selected delete.Click the button  to delete the diagnostic software.

|  |
| --- |
| AppsApps1 |

### 4.13.3 Video Management

Users can not only browse video but also delete video, including single deletion, multiple deletions, or all deletions.

Click the Video to browse the Video. Click the button  to delete the Video.

|  |
| --- |
| videovideo 1 |

### 4.13.4 Report Management

Users can not only browse report but also delete report, including single deletion, multiple deletions, or all deletions.

Click the Report to browse the Report. Click the button  to delete the Report.

|  |
| --- |
| reportcopytoqq |

## 4.14 User Management

Input workshop information, and chick the button  to save the information.

Click the button  to change the information.

|  |
| --- |
| 图片1_副本user 1_副本 |

## 4.15 Quick Support

Run “Quick Support”to receive remote support.

|  |
| --- |
| 主界面0 |

# 5. Products Website

Please focus on our website [www.IDUTEX.com](http://www.tdintel.com) for the updating information and other news.

# 6. Warranty

Vpecker software is free updating within 1 year from the date of product activation.