**How to Update SEC-E9 key cutting machine**

**----For 8″ inch Tablet PC version**

New customers need to [register](http://user.kkkcut.com/en/Register.aspx) to Hunan kukai’s membership system first.

Old customers please [login](http://user.kkkcut.com/en/Login.aspx) the membership system.

How to upgrade:



Login to membership system.



Check upgrade information and latest database available



Download database to your computer



Unzip database



Insert USB disk with database to [SEC-E9 key cutting machine](http://www.obdii365.com/wholesale/sec-e9-cnc-key-cutting-machine.html)



Go to Device setup->Upgrade



Wait until upgrade is finished.

**How to upgrade SEC-E9 key cutting machine?**

**—for Tablet PC Bluetooth Version**

1. Click ”Setup”



2. Click”Wifi”



3. Connect Wifi

4. Press ”UpdateCheck” after the wifi is connected successfully.

( Please notice that you just need to click the ”UpdateCheck” once, no need to click it repeatedly)



5. Click ”Upgrade” button



6. After upgrading successfully, the tablet PC will automatically jump to the main page.



Notice

1. Please keep the **Wifi connected** when upgrade

2. Please keep the **network smooth**

3. Please **do not turn off tablet PC** when upgrading

4. Please **do not operate the tablet PC** when downloading the upgrade files.

5. Please **disconnect Wifi** after upgrade is done. ( otherwise the system will generate garbage when tablet PC updates automatically . Also cause the system to run slowly.)